This folder contains the positive gerber versions (G1 and G2) of the negative power plane gerbers (GP1 and GP2). **It is important to note that we have not yet used these positive gerbers to fabrication the DAQ PCB. Use at your own risk.**

* USB\_Control.G1 is the positive gerber of USB\_Control.GP1
* USB\_Control.G2 is the positive gerber of USB\_Control.GP2
* Order of copper layers:
  + Component layer (Top Layer)
  + Ground plane (GP1 or G1)
  + Power plane (GP2 or G2)
  + Signal layer (Bottom Layer)